<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<library>
<packages>
<package name="MO-187AA">
<description>
&lt;b&gt;Plastic Shrink Small Outline Package&lt;/b&gt;, 3mm x 3mm body, 0.65mm lead pitch&lt;p&gt;
JEDEC MO-187, variation AA&lt;br&gt;
land pattern recommendation: NS (MUA08A)&lt;p&gt;
Analog Devices: MSOP08&lt;br&gt;
Maxim: µMAX8 (uMAX8)&lt;br&gt;
Microchip: MSOP8&lt;br&gt;
National Semiconductor: MUA08A&lt;br&gt;
NXP: TSSOP8 (SOT505)&lt;br&gt;
ON: Micro8&lt;br&gt;
Texas Instruments: VSSOP8 (DGK, S-PDSO-G8)&lt;br&gt;
Vishay: MSOP8&lt;br&gt;
</description>
</package>
<package name="SOT23-6">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; 6 lead</description>
</package>
<package name="ML10">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
<package name="ML10L">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
<package name="3M_10">
<description>&lt;b&gt;3M&lt;/b&gt;</description>
</package>
<package name="3M_10L">
<description>&lt;b&gt;3M&lt;/b&gt;</description>
</package>
<package name="D2PAK5_12345_(ON)">
<description>
&lt;b&gt;Small outline transistor&lt;/b&gt;, pad names 1-2-3-4-5, reflow soldering&lt;p&gt;
Source of package/pad dimensions: ON&lt;p&gt;
other notations:&lt;ul&gt;
&lt;li&gt;D2PAK-5, D2PAK/5, D2-PAK5, D2-PAK-5, D2-PAK/5
&lt;li&gt;DDPAK5, DDPAK-5, DDPAK/5
&lt;li&gt;DD-PAK5, DD-PAK-5, DD-PAK/5
&lt;li&gt;TO263-5, TO-263-5, TO263/5, TO-263/5
&lt;/ul&gt;
</description>
</package>
<package name="78XXL">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="78XXS">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="TO252">
</package>
<package name="TO263">
<description>&lt;b&gt;TO-263 Package&lt;/b&gt;</description>
</package>
<package name="SOT223">
</package>
<package name="JUMPER_3W">
</package>
<package name="1X02-S">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="JUMPER_4W">
</package>
</packages>
<symbols>
<symbol name="TCA9803">
<pin name="VCCA" direction="pwr"/>
<pin name="SCLA"/>
<pin name="SDAA"/>
<pin name="GND" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="SDAB"/>
<pin name="SCLB"/>
<pin name="VCCB" direction="pwr"/>
</symbol>
<symbol name="SN74AXC1T45">
<pin name="VCCA" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A"/>
<pin name="B"/>
<pin name="DIR" direction="in"/>
<pin name="VCCB" direction="pwr"/>
</symbol>
<symbol name="SN74AXC2T45">
<pin name="VCCA" direction="pwr"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="GND" direction="pwr"/>
<pin name="DIR" direction="in"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="VCCB" direction="pwr"/>
</symbol>
<symbol name="10P">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="BEAGLECONN">
<pin name="SCL" direction="pas"/>
<pin name="GND@2" direction="pas"/>
<pin name="SDA" direction="pas"/>
<pin name="TPWR@4" direction="pas"/>
<pin name="SDI" direction="pas"/>
<pin name="TPWR@6" direction="pas"/>
<pin name="SCK" direction="pas" function="clk"/>
<pin name="SDO" direction="pas"/>
<pin name="CS#" direction="pas" function="dot"/>
<pin name="GND@10" direction="pas"/>
</symbol>
<symbol name="LP38502">
<pin name="IN" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="sup"/>
</symbol>
<symbol name="78XX">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="TAB" direction="pas"/>
</symbol>
<symbol name="JUMPER_3WAY">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="C"/>
</symbol>
<symbol name="JUMPER_4WAY">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="C"/>
<pin name="4"/>
</symbol>
<symbol name="+3V3">
<pin name="+3V3" direction="sup"/>
</symbol>
<symbol name="+1V8">
<pin name="+1V8" direction="sup"/>
</symbol>
<symbol name="+1V2">
<pin name="+1V2" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TCA9803DGK">
<gates>
<gate name="G$1" symbol="TCA9803"/>
</gates>
<devices>
<device name="" package="MO-187AA">
<connects>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCLA" pad="2"/>
<connect gate="G$1" pin="SCLB" pad="7"/>
<connect gate="G$1" pin="SDAA" pad="3"/>
<connect gate="G$1" pin="SDAB" pad="6"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74AXC1T45DBV">
<gates>
<gate name="G$1" symbol="SN74AXC1T45"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="4"/>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74AXC2T45DCU">
<gates>
<gate name="G$1" symbol="SN74AXC2T45"/>
</gates>
<devices>
<device name="" package="MO-187AA">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="B1" pad="7"/>
<connect gate="G$1" pin="B2" pad="6"/>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCCA" pad="1"/>
<connect gate="G$1" pin="VCCB" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ML10" prefix="SV" uservalue="yes">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="10P"/>
</gates>
<devices>
<device name="" package="ML10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L" package="ML10L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BEAGLECONN">
<gates>
<gate name="G$1" symbol="BEAGLECONN"/>
</gates>
<devices>
<device name="" package="ML10">
<connects>
<connect gate="G$1" pin="CS#" pad="9"/>
<connect gate="G$1" pin="GND@10" pad="10"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="SCK" pad="7"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SDI" pad="5"/>
<connect gate="G$1" pin="SDO" pad="8"/>
<connect gate="G$1" pin="TPWR@4" pad="4"/>
<connect gate="G$1" pin="TPWR@6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP38502">
<gates>
<gate name="G$1" symbol="LP38502"/>
</gates>
<devices>
<device name="" package="D2PAK5_12345_(ON)">
<connects>
<connect gate="G$1" pin="ADJ" pad="5"/>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="GND" pad="3.1 3.2"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="TAB" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER_3WAY">
<gates>
<gate name="G$1" symbol="JUMPER_3WAY"/>
</gates>
<devices>
<device name="" package="JUMPER_3W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JUMPER_4WAY">
<gates>
<gate name="G$1" symbol="JUMPER_4WAY"/>
</gates>
<devices>
<device name="" package="JUMPER_4W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+3V3" prefix="+3V3">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="+3V3"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+1V8">
<gates>
<gate name="G$1" symbol="+1V8"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+1V2">
<gates>
<gate name="G$1" symbol="+1V2"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
